GPS CPIT GP-27

This GPS was created without protection code (if bought after 10 July 2005) to solve several issues existing between the several Nemerix GPS receivers on sale, and the bluetooth devices containing the navigation software. So don’t try to pair the GPS with your PDA or smartphone.

Details:

RED LED: Battery status (red light always standing on)

GREEN LED: GPS signal status (slow flashing: no GPS signal available – fast flashing: GPS signal available)

BLUE LED: Bluetooth connection status (fast flashing: no devices connected – slow flashing: the GPS receiver is trying to make a connection with a Bluetooth device – blue light standing on: Bluetooth connection activated)

GPS configuration with TomTom Mobile 5 and Route 66:

1) Turn on the GPS receiver and wait until it catches the signal (the green led must flash fastly). The blue led flashes fast too (no devices connected).

2) Run TomTom Mobile 5

3) Execute: Menu ( Change Preferences ( Show GPS status ( Configure ( Choose Other Bluetooth GPS and Select.

4) Now we need to find the cpit-GPS. Start to search Bluetooth devices (if in the start you see no devices persist until you see the GPS device), choose cpit-GPS, then select it and press Done. Exit the program. While your exit you should see the blue led flashing slower than before. The pairing is done.

5) Then (and for the following times) execute only the steps 1) and 2) and just wait till the blue led flashes slowly (if your device ask you the protection code, ignore it). Follow then the step 3) and choose the cpit-GPS already standing in the list; the blue light will turn always on without flashing and you should see the GPS signal shown on the display. Done (
For the navigation program Route 66 Mobile follow the step 1), run the program and choose cpit-GPS as default GPS devide. Restart the program and it’s done. The following times the connection will be automatic.

For the other devices the procedure should not be much different.
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